Rename the unforce_pulse4kmini.txt to force_pulse4kmini.txt and move it to the root of your usb-stick
When you enter the recovery menu then it will then force the openvix-6.8.008.release-pulse4kmini_mmc.zip into the linux1 slot
